

All loads containing biohazardous waste must be autoclaved at 121°C for a minimum of 30 minutes. 7/2020

**AUTOCLAVE LOG SHEET**

|  |  |  |  |
| --- | --- | --- | --- |
| **Autoclave make/model:** |  | **Location****(building/room number):** |  |
| **Lab/Facility name:** |  | **Principal Investigator/****Supervisor name:** |  |
| **Person responsible for autoclave:** |  | **Phone number:** |  |
| Date | Contents | Cycle Number | Cycle Type | Sterilization Time (min) | Pressure (psi) | Max Temp Reached | Tape Result (pass/fail) | Chemical Integrator Result(pass/fail) | Biological Indicator Used?(Y/N) | Operator | Comments |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |